Cannondale scalpel si black inc 2018

$ 12.694,17

Frame scalpel-si, 100mm, ballistec hi-mod carbon, zero pivot seatstay, pf30, 1.5 si head tube, ai offset

Fork lefty 2.0 carbon, 100mm, xlr isolated damper technology with xc+ tune and xloc full sprint remote, 55mm offset

Rear shock rockshox monarch xx, 100mm, full sprint remote

Rims enve carbon m50, tubeless ready,28h

Hubs lefty 60 front, chris king iso rear, 142x12, 28 hole (ai offset dish - rear)

Spokes  dt swiss aerolite (ai offset dish - rear)

Tires schwalbe racing ralph evo snakeskin, 29x2.25", folding, tubeless ready

Pedals n/a

Crank cannondale hollowgram sisl2, hollow forged, bb30, 32t ai spidering

Bottom bracket cannondale alloy pressfit30

Chain shimano cn-hg901, 11-speed

Rear cogs shimano xtr, 11-40, 11-speed

Front derailleur shimano xtr di2, direct mount, 2x

Rear derailleur shimano xtr di2, 11-speed

Shifters shimano xtr di2, 2x11

Handlebar enve carbon sweep, flat, 740mm

Grips cannondale locking grips

Stem cannondale c1, 6061 alloy, 1.5", 31.8, -5 deg.

Headset cannondale headshok si

Brakes shimano xtr race, 160/160mm, ice tech rotors

Brake levers shimano xtr race, carbon lever

Saddle prologo zero ii cpc nack carbon

Seatpost enve carbon, di2 compatible, 31.6x400mm

Sizes s (27.5") m,l,xl (29")

Specialized stumpjumper fsr expert carbon 29 – 2017

$5,000.00

Frame

Specialized fact 9m, carbon front chassis, m5 alloy rear end, trail geometry, swat™ door integration, pf30 bb, fully enclosed internal cable routing,

Manfu link, 12x148mm dropouts, sealed cartridge bearing pivots, replaceable derailleur hanger, 135mm of travel

Fork

Rockshox pike rc 29/27.5+, solo air, compression and rebound adjust, tapered steerer, 15x110mm maxle stealth thru-axle, 51mm offset, 150mm travel

Rear shock

Rockshox monarch rt3, rx trail tune, autosag, rebound and 3-position compression adjust, 197x48mm

Rims/wheels

Roval traverse 29, 29mm internal width

Hubs

Roval traverse

Spokes

Dt swiss revolution

Tires

Specialized 2bliss ready 29 x 2.3 front: butcher rear: slaughter

Crankset

Raceface aeffect

Rear

Derailleur

Sram x1

Rear cogs

Sram xg-1150, 11-speed, 10-42t

Shifters

Sram gx

Handlebars

Specialized trail

Tape/grips

Specialized sip grip

Stem

Specialized trail, aluminum

Brakes

Sram guide r, hydraulic disc, front: 200/180mm; rear: 180/160mm

Saddle

Specialized body geometry henge comp, 143mm wide

Seatpost

Specialized command post ircc, 12 position micro-height adjustable, alien head design, bottom mount cable routing, remote srl lever, 30.9mm, s: 100mm,

M/l/xl: 125mm travel

Giant Anthem advanced pro 29 0

2018

$8,670

Sizes s, m, l, xl

Colors matte carbon smoke/gloss blue/gloss dark blue

Frame advanced-grade composite mainframe and rear triangle, advanced forged composite upper rocker, 90mm maestro suspension

Fork fox 32 float sc factory remote, fit4 damper, remote lockout, boost, kabolt, overdrive, 100mm travel

Shock fox float factory remote, trunnion mount

Handlebar giant contact slr trail, composite

Stem giant contact slr, composite

Seatpost giant contact slr, composite, 27.2mm

Saddle giant contact slr, forward

Pedals n/a

Shifters sram xx1 eagle

Front derailleur n/a

Rear derailleur sram xx1 eagle, type 2

Brakes sram level ultimate, hydraulic disc, [f] 180mm, [r] 160mm

Brake levers sram level ultimate

Cassette sram xx1 eagle, 10x50, 12-speed

Chain sram xx1 eagle

Crankset sram xx1 eagle carbon, 34t

Bottom bracket sram gxp, press fit

Rims giant xcr 0 29 composite dbl wheelsystem; 27mm wide, tubeless

Hubs giant xcr 0 29 composite dbl wheelsystem; star ratchet driver, boost

Spokes giant xcr 0 29 composite dbl wheelsystem; dynamic balanced lacing, dt swiss aerolite bladed stainless

Tires maxxis ikon 29x2.2, folding, 120 tpi, 3c, exo, tubeless

Extras factory tubeless

Weight the most accurate way to determine any bike’s weight is to have your local dealer weigh it for you. Many brands strive to list the lowest possible weight, but in reality weight can vary based on size, finish, hardware and accessories. All giant bikes are designed for best-in-class weight and ride quality.